|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **LJBL** | | | | | | **BLED, SLOVENIA** | | | | | | | | | | | | | | |
| *Apt Elev* **1654’**/504m  N46°21’23’’ E014°10’28’’ | | | | | | | | | 2021-03-25 | | | | LESCE | | | | | | | |
| AIR/GND | | | | LESCE BLED AERODROME  **122.505 MHz** | | | | | | | FIS | | | | | LJUBLJANA INFO  **118.480 MHz** | | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | **DIMENSION** | | | | **SURFACE** | | **TORA** | | | **TODA** | | | | **ASDA** | | | **LDA** | **LIGHTS** | **PATTERN** |
| 14 | | 1130 x 23 m | | | | asphalt | | 1130 | | | 1130 | | | | 1130 | | | 955 | nil | LH & RH |
| 32 | |  | | | |  | | 955 | | | 955 | | | | 1130 | | | 1130 |  | LH & RH |
| 14 | | 600 x 30 m | | | | grass | | 600 | | | 600 | | | | 600 | | | 600 | nil | LH & RH |
| 32 | |  | | | |  | | 600 | | | 600 | | | | 600 | | | 600 |  | LH & RH |
|  | | | | | | | | | | | | | | | | | | | | |
| **NOTES:**  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome operations manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021. | | | | | | | | | | | | | | | | | | | | |
| **LJBL** | | | | | | | **BLED, SLOVENIA** | | | | | | | | | | | | | |
| *Apt Elev* **1654’**/504m  N46°21’23’’ E014°10’28’’ | | | | | | | 2021-03-25 | | | | | | | | LESCE | | | | | |
| AIR/GND | | LESCE BLED AERODROME  **122.505 MHz** | | | | | | | FIS | | | | LJUBLJANA INFO  **118.480 MHz** | | | | | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous radio watch.** 2. **Public lighting and trees 340 m before threshold 14.** 3. **Public lighting 320 m, trees and electric landline 1000 m SE from threshold 32.** | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – prior permission required. 2. Only VFR flights allowed. Simultaneous operations on both runways are prohibited. 3. Only for ACFT with MTOW < 5700 kg. 4. Often parachuting activity. Helicopter operations allowed NE of runway only. 5. Overflying residential areas in the vicinity should be avoided. | | | | | | | | | | | | | | | |
| **Operator** | | | | Alpski letalski center | | | | | | | **Email** | | | | | info@alc-lesce.si | | | |
| **Address** | | | | Begunjska 10 | | | | | | | **Internet** | | | | | http://www.alc-lesce.si | | | |
| **Zip City** | | | | SI-4248 Lesce | | | | | | | **ARO** | | | | | +386 4 2040 420 – Ljubljana | | | |
| **Tel** | | | | +386 4 5320 100 | | | | | | | **METEO** | | | | | +386 4 2804 500 – Ljubljana | | | |
| **Fax** | | | | +386 4 5320 101 | | | | | | | **Customs** | | | | | N/A | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021.

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-03-25 | Initial version |