|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **LJMS** | | | | | | **MURSKA SOBOTA, SLOVENIA** | | | | | | | | | | | | | | |
| *Apt Elev* **604’**/184m  N46°37’50’’ E16°10’37’’ | | | | | | | | | 2021-03-25 | | | | RAKIČAN | | | | | | | |
| AIR/GND | | | | SOBOTA AERODROME  **123.505 MHz** | | | | | | | APP | | | | | MARIBOR APPROACH  **119.205 MHz** | | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | **DIMENSION** | | | | **SURFACE** | | **TORA** | | | **TODA** | | | | **ASDA** | | | **LDA** | **LIGHTS** | **PATTERN** |
| 09 | | 1050 x 76 m | | | | grass | | 1050 | | | 1050 | | | | 1050 | | | 1050 | nil | RH (& LH\*) |
| 27 | |  | | | |  | | 1050 | | | 1050 | | | | 1050 | | | 1050 |  | LH (& RH\*) |
| 01 | | 850 x 56 m | | | | grass | | 850 | | | 850 | | | | 850 | | | 850 | nil | LH & RH |
| 19 | |  | | | |  | | 850 | | | 850 | | | | 850 | | | 850 |  | LH & RH |
|  | | | | | | | | | | | | | | | | | | | | |
| **NOTES:** \* Traffic pattern for gliders  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome operations manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021. | | | | | | | | | | | | | | | | | | | | |
| **LJMS** | | | | | | | **MURSKA SOBOTA, SLOVENIA** | | | | | | | | | | | | | |
| *Apt Elev* **604’**/184m  N46°37’50’’ E16°10’37’’ | | | | | | | 2021-03-25 | | | | | | | | RAKIČAN | | | | | |
| AIR/GND | | SOBOTA AERODROME  **123.505 MHz** | | | | | | | APP | | | | MARIBOR APPROACH  **119.205 MHz** | | | | | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous radio watch.** | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – prior permission required at least 2h before arrival. 2. Only VFR flights allowed. 3. Large trees penetrating approach/take-off and side surfaces of RWY 01/19. 4. Flying below 3000ft QFE overhead hospital prohibited 5. MTOM 12 tons. 6. Often gliding, skydiving and aerobatic activity. | | | | | | | | | | | | | | | |
| **Operator** | | | | Aeroklub Murska Sobota | | | | | | | **Email** | | | | | info@aeroklub-ms.si | | | |
| **Address** | | | | Muzge 2 | | | | | | | **Internet** | | | | | http://www.aeroklub-ms.si | | | |
| **Zip City** | | | | SI-9000 Murska Sobota, | | | | | | | **ARO** | | | | | +386 4 2040 420 – Ljubljana | | | |
| **Tel** | | | |  | | | | | | | **METEO** | | | | | +386 2 6296 871 – Maribor | | | |
| **Fax** | | | |  | | | | | | | **Customs** | | | | | N/A | | | |
| **Mobile** | | | |  | | | | | | | **Fuel** | | | | | N/A | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021.

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-03-25 | Initial version |