|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **LJSG** | | | | | | **SLOVENJ GRADEC, SLOVENIA** | | | | | | | | | | | | | | |
| *Apt Elev* **1644’**/501m  N46°28’18’’ E015°07’03’’ | | | | | | | | | 2021-03-25 | | | | MISLINJSKA DOBRAVA | | | | | | | |
| AIR/GND | | | | SLOVENJ GRADEC AERODROME  **123.505 MHz** | | | | | | | FIS | | | | | LJUBLJANA INFO  **118.480 MHz** | | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | **DIMENSION** | | | | **SURFACE** | | **TORA** | | | **TODA** | | | | **ASDA** | | | **LDA** | **LIGHTS** | **PATTERN** |
| 14 | | 1200 x 23 m | | | | asphalt | | 1200 | | | 1200 | | | | 1200 | | | 1100 | nil | LH (RH\*) |
| 32 | |  | | | |  | | 1200 | | | 1200 | | | | 1200 | | | 1200 |  | RH (LH\*) |
| 14 R | | 650 x 30 m | | | | grass | | 650 | | | 650 | | | | 650 | | | 650 | nil | LH (RH\*) |
| 32 L | |  | | | |  | | 650 | | | 650 | | | | 650 | | | 650 |  | RH (LH\*) |
|  | | | | | | | | | | | | | | | | | | | | |
| **NOTES:** \* Traffic pattern for gliders  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome operations manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021. | | | | | | | | | | | | | | | | | | | | |
| **LJSG** | | | | | | | **SLOVENJ GRADEC, SLOVENIA** | | | | | | | | | | | | | |
| *Apt Elev* **1644’**/501m  N46°28’18’’ E015°07’03’’ | | | | | | | 2021-03-25 | | | | | | | | MISLINJSKA DOBRAVA | | | | | |
| AIR/GND | | SLOVENJ GRADEC AERODROME  **123.505 MHz** | | | | | | | FIS | | | | LJUBLJANA INFO  **118.480 MHz** | | | | | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous radio watch.** | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – prior permission required. | | | | | | | | | | | | | | | |
| **Operator** | | | | Aerodrom Slovenj Gradec d.o.o. | | | | | | | **Email** | | | | | ljsg.info@gmail.com | | | |
| **Address** | | | | Mislinjska Dobrava 110 | | | | | | | **Internet** | | | | |  | | | |
| **Zip City** | | | | SI-2383 Šmartno pri Slovenj Gradcu | | | | | | | **ARO** | | | | | +386 4 2040 420 – Ljubljana | | | |
| **Tel** | | | | +386 2 8855 502 | | | | | | | **METEO** | | | | | +386 4 2804 500 – Ljubljana | | | |
| **Fax** | | | |  | | | | | | | **Customs** | | | | | N/A | | | |
| **Mobile** | | | |  | | | | | | | **Fuel** | | | | | 100 LL, JET A1, NMB95 octane | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021.

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-03-25 | Initial version |