|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **LJSO** | | | | | | **ŠOŠTANJ, SLOVENIA** | | | | | | | | | | | | | | |
| *Apt Elev* **1239’**/378m  N46°23’53’’ E015°02’42’’ | | | | | | | | | 2021-03-25 | | | | LAJŠE | | | | | | | |
| AIR/GND | | | | ŠOŠTANJ AERODROME  **128.305 MHz** | | | | | | | FIS | | | | | LJUBLJANA INFO  **118.480 MHz** | | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | **DIMENSION** | | | | **SURFACE** | | **TORA** | | | **TODA** | | | | **ASDA** | | | **LDA** | **LIGHTS** | **PATTERN** |
| 15 | | 714 x 18 m | | | | asphalt | | 714 | | | 714 | | | | 714 | | |  | nil | T/O only |
| 33 | |  | | | |  | |  | | |  | | | |  | | | 714 |  | LND only |
|  | | | | | | | | | | | | | | | | | | | | |
| **NOTES:**  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome operations manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021. | | | | | | | | | | | | | | | | | | | | |
| **LJSO** | | | | | | | **ŠOŠTANJ, SLOVENIA** | | | | | | | | | | | | | |
| *Apt Elev* **1239’**/378m  N46°23’53’’ E015°02’42’’ | | | | | | | 2021-03-25 | | | | | | | | LAJŠE | | | | | |
| AIR/GND | | ŠOŠTANJ AERODROME  **128.305 MHz** | | | | | | | FIS | | | | LJUBLJANA INFO  **118.480 MHz** | | | | | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous radio watch.** 2. **Take off using RWY 33 strictly prohibited due to terrain.** 3. **Landing using RWY 15 strictly prohibited due to terrain.** | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – prior permission required. 2. Only VFR flights allowed. 3. Large trees penetrating left side surface along RWY 33. | | | | | | | | | | | | | | | |
| **Operator** | | | | Šaleški aeroklub | | | | | | | **Email** | | | | | zvonimir.mavri@gmail.com | | | |
| **Address** | | | | Topolšica 207c, | | | | | | | **Internet** | | | | | http://www.saleskiaeroklub.si | | | |
| **Zip City** | | | | SI-3325 Šoštanj | | | | | | | **ARO** | | | | | +386 4 2040 420 – Ljubljana | | | |
| **Tel** | | | | +386 3 589 23 06 | | | | | | | **METEO** | | | | | +386 4 2804 500 – Ljubljana | | | |
| **Fax** | | | | +386 3 589 23 01 | | | | | | | **Customs** | | | | | N/A | | | |
| **Mobile** | | | |  | | | | | | | **Fuel** | | | | | N/A | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. 2021.

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-03-25 | Initial version |