|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| [Abstract] | | | | | | **KAMNIK, SLOVENIA** | | | | | | | | | | | | | | | | | | | |
| *Apt Elev* **1145’**/349m  N46°11’50’’ E014°34’51’’ | | | | | | | | | | | 2021-04-22 | | | | | DUPLICA | | | | | | | | | |
| AIR/GND | | KAMNIK AIRFIELD  **123.505** | | | | | FIS | | | | | LJUBLJANA INFO  **118.480** | | | | | | | TWR | | | LJUBLJANA TOWER  **118.005** | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | | | **DIMENSION** | | **SURFACE** | | | | **TORA** | | | | **TODA** | | | **ASDA** | | | | **LDA** | | | **LIGHTS** | **PATTERN** |
| 11 | | | | 425 x 25 m | | grass | | | |  | | | |  | | |  | | | | 425 | | | nil | LND only |
| 29 | | | | 425 | | | | 425 | | | 425 | | | |  | | | T/O only |
|  | | | | | | | | | | | | | | | | | | | | | | | | | |
| **NOTES:**  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. www.vfr-charts.ga | | | | | | | | | | | | | | | | | | | | | | | | | |
| [Abstract] | | | | | | | | | **KAMNIK, SLOVENIA** | | | | | | | | | | | | | | | | |
| *Apt Elev* **1145’**/349m  N46°11’50’’ E014°34’51’’ | | | | | | | | | 2021-04-22 | | | | | | | | DUPLICA | | | | | | | | |
| AIR/GND | | KAMNIK AIRFIELD  **123.505** | | | | | FIS | | | | | LJUBLJANA INFO  **118.480** | | | | | | | TWR | | | LJUBLJANA TOWER  **118.005** | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous airfield radio watch. Transmit blind.** 2. **On board radio mandatory.** 3. **Airstrip is located within CTR Ljubljana. Clearance to enter the airspace must be obtained from corresponding ATS (Ljubljana TWR).** 4. **Power lines 342 m and 366 m E of threshold RWY 29 (height 10 m and 35 m).** | | | | | | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – prior permission required. 2. Traffic pattern height is maximum 150 ft AGL or as obtained from ATS. 3. Only VFR flights allowed. | | | | | | | | | | | | | | | | | | | | |
| **Operator** | | | | Letalski klub Kamnik | | | | | | | | | | **Email** | | | letalski.klub.kamnik@gmail.com | | | | | | | |
| **Address** | | | | Korenova ulica 9a | | | | | | | | | | **Internet** | | | http://www.vzletisce-kamnik.si | | | | | | | |
| **Zip City** | | | | SI-1241 Kamnik | | | | | | | | | | **ARO** | | | +386 4 2040 420 – Ljubljana | | | | | | | |
| **Mobile** | | | | +386 31 878 645 | | | | | | | | | | **METEO** | | | +386 4 2804 500 – Ljubljana | | | | | | | |
| **Tel** | | | |  | | | | | | | | | | **Customs** | | | N/A | | | | | | | |
| **Fax** | | | |  | | | | | | | | | | **Fuel** | | | N/A | | | | | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. www.vfr-charts.ga

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-04-22 | Initial version |