|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| [Abstract] | | | | | | **KOČEVJE, SLOVENIA** | | | | | | | | | | | | | | |
| *Apt Elev* **1765’**/538m  N45°34’12’’ E014°51’30’’ | | | | | | | | | 2021-07-15 | | | | NOVI LAZI – KOČEVSKA REKA | | | | | | | |
| AIR/GND | | | | KOČEVJE AIRFIELD  **123.505** | | | | | | | FIS | | | | | LJUBLJANA INFO  **118.480** | | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | **DIMENSION** | | | | **SURFACE** | | **TORA** | | | **TODA** | | | | **ASDA** | | | **LDA** | **LIGHTS** | **PATTERN** |
| 15 | | 300 x 30 m | | | | grass | | 300 | | | 300 | | | | 300 | | | 300 | nil | LH & RH |
| 33 | |  | | | |  | | 300 | | | 400 | | | | 300 | | | 300 |  | LH & RH |
|  | | | | | | | | | | | | | | | | | | | | |
| **NOTES:**  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. www.vfr-charts.ga | | | | | | | | | | | | | | | | | | | | |
| [Abstract] | | | | | | | **KOČEVJE, SLOVENIA** | | | | | | | | | | | | | |
| *Apt Elev* **1765’**/538m  N45°34’12’’ E014°51’30’’ | | | | | | | 2021-07-15 | | | | | | | | NOVI LAZI – KOČEVSKA REKA | | | | | |
| AIR/GND | | KOČEVJE AIRFIELD  **123.505** | | | | | | | FIS | | | | LJUBLJANA INFO  **118.480** | | | | | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous radio watch. Transmit blind.** 2. **Avoid flying over populated areas – villages Štalcarji and Novi Lazi.** 3. **Pay attention to the road before threshold 15.** | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – Prior permission required. 2. Only VFR flights allowed. 3. 100 m clearway marked with yellow flags located behind the departure end of runway 33 which is hardened and maintained the same way as main runway. | | | | | | | | | | | | | | | |
| **Operator** | | | | Letalski klub Kočevje | | | | | | | **Email** | | | | | lk.kocevje@gmail.com | | | |
| **Address** | | | | Pri Unionu 16 | | | | | | | **Internet** | | | | | www.lk-kocevje.si | | | |
| **Zip City** | | | | SI-1330 Kočevje | | | | | | | **ARO** | | | | | +386 4 2040 420 – Ljubljana | | | |
| **Tel** | | | |  | | | | | | | **METEO** | | | | | +386 4 2804 500 – Ljubljana | | | |
| **Fax** | | | |  | | | | | | | **Customs** | | | | | N/A | | | |
| **Mobile** | | | | +386 41 430 745 | | | | | | | **Fuel** | | | | | N/A | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. www.vfr-charts.ga

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-07-15 | Initial version |