|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| [Abstract] | | | | | | **PODČETRTEK, SLOVENIA** | | | | | | | | | | | | | | | | | | | |
| *Apt Elev* **645’**/197m  N46°07’37’’ E015°36’14’’ | | | | | | | | | | | 2021-05-20 | | | | | IMENO | | | | | | | | | |
| AIR/GND | | IMENO AIRFIELD  **123.505** | | | | | APP | | | | | CERKLJE APPROACH  **118.555** | | | | | | | FIS | | | LJUBLJANA INFO  **118.480** | | | |
| **Visual Approach Chart** | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | |
| **RWY** | | | | **DIMENSION** | | **SURFACE** | | | | **TORA** | | | | **TODA** | | | **ASDA** | | | | **LDA** | | | **LIGHTS** | **PATTERN** |
| 01 | | | | 600 x 30 m | | grass | | | | 600 | | | | 600 | | | 600 | | | | 600 | | | nil | RH |
| 19 | | | | 600 | | | | 600 | | | 600 | | | | 600 | | | LH |
|  | | | | | | | | | | | | | | | | | | | | | | | | | |
| **NOTES:**  All the distances in meters. Not for official use. All data for information purposes only. Check latest info in official aerodrome manual and AIP before commencing any flight. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. www.vfr-charts.ga | | | | | | | | | | | | | | | | | | | | | | | | | |
| [Abstract] | | | | | | | | | **PODČETRTEK, SLOVENIA** | | | | | | | | | | | | | | | | |
| *Apt Elev* **645’**/197m  N46°07’37’’ E015°36’14’’ | | | | | | | | | 2021-05-20 | | | | | | | | IMENO | | | | | | | | |
| AIR/GND | | IMENO AIRFIELD  **123.505** | | | | | APP | | | | | CERKLJE APPROACH  **118.555** | | | | | | | FIS | | | LJUBLJANA INFO  **118.480** | | |
| **Ground Movement Chart** | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | |
| **Warnings** | | | | 1. **No continuous radio watch. Transmit blind.** 2. **Western traffic pattern only.** 3. **Pay attention to the border with Croatia.** 4. **Minimum traffic pattern altitude is 1650 ft due to terrain.** | | | | | | | | | | | | | | | | | | | | |
| **Remarks** | | | | 1. PPR – Prior permission required. 2. Only VFR flights allowed. | | | | | | | | | | | | | | | | | | | | |
| **Operator** | | | | Obsoteljski Aeroklub Imeno | | | | | | | | | | **Email** | | | info@aeroklub-imeno.si | | | | | | | |
| **Address** | | | | Olimje 6 | | | | | | | | | | **Internet** | | | www.aeroklub-imeno.si | | | | | | | |
| **Zip City** | | | | SI-3254 Podčetrtek | | | | | | | | | | **ARO** | | | +386 4 2040 420 – Ljubljana | | | | | | | |
| **Mobile** | | | |  | | | | | | | | | | **METEO** | | | +386 4 2804 500 – Ljubljana | | | | | | | |
| **Tel** | | | |  | | | | | | | | | | **Customs** | | | N/A | | | | | | | |
| **Fax** | | | |  | | | | | | | | | | **Fuel** | | | N/A | | | | | | | |

Not for official use. All data for information purposes only. Copyleft Small letter c turned 180 degrees, surrounded by a single line forming a circle. www.vfr-charts.ga

|  |  |  |
| --- | --- | --- |
| **SYMBOL LEGEND** | | |
|  | | |
| **Revision history** | | |
| **Revision** | **Date** | **Changes** |
| v1 | 2021-05-20 | Initial version |